




VLIHubPDUpdateTool Installation and FW update Tutorial


The following describes how to install VLIHubPDUpdateTool and update FW. PC system need to be Windows.


1. **Open the “****VLIHubPDUpdateTool” installation package, locate “VLIHubPDUpdateTool\_v1.0.1.7\_install\_07272021.exe”, and click to open it:** 
2. **The following windows appear, click "Next".** 







**3.The following window appears, click "Install" and wait until the installation progress is complete.**






**4.The following window appears. Select“Yes, restart the computer now” and click “Finish” to restart the PC. After that “VLIHubPDUpdateTool” can be used.**  

**5.Connect the docking to the PC, then open the “VLIHubPDUpdateTool”, and click “Upgrade FW” in the following window.**





**6. The following window appears, which means the FW update is completed, then click “确定/OK/Finish” .**

